***Power & Hand Tool Focus Inspection – Site-specific Hazard Assessment for New Tool Checklist***

**Date:\_\_\_\_\_\_\_\_\_\_\_\_\_ Foreman:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ General Foreman:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Superintendent:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

|  |  |  |
| --- | --- | --- |
| **Craft:** | **Inspector:** | **Area:** |
| **Items for Inspection** | **\*C** | **\*\*NC** | **ID** | **Comments** | Supervisor / Trade / Position |
| **General – Power Tools** |
| * UL or CSA approved
 |  |  |  |  |  |
| * Proper attachments for tool
 |  |  |  |  |  |
| * Side handle used
 |  |  |  |  |  |
| * Disconnect whenadjusted
 |  |  |  |  |  |
| * Foot pedal installed
 |  |  |  |  |  |
| * Trigger locks removed
 |  |  |  |  |  |
| * Proper guards installed
 |  |  |  |  |  |
| **General – Hand Tools** |
| * Tie backs (drop hazard)
 |  |  |  |  |  |
| * Carried in pouch
 |  |  |  |  |  |
| * Handle in good repair
 |  |  |  |  |  |
| * Handles on file
 |  |  |  |  |  |
| * Ladders (C.C.)
 |  |  |  |  |  |
| * No snipes
 |  |  |  |  |  |
| **Knives/Cutting tools** |
| * No razor knives
 |  |  |  |  |  |
| * Striking tool dressed
 |  |  |  |  |  |
| **Sub-Totals** |  |  |  | **Imminent Danger = -20% off total score** % Compliance = (In Compliance X 100) / Total  |
| **Total Values (Combined)** |  | **% Compliance This Week**:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |  |